Object = IsisCube
  Object = Core
    StartByte   = 65537
    Format      = Tile
    TileSamples = 128
    TileLines   = 128

    Group = Dimensions
      Samples = 959
      Lines   = 1404
      Bands   = 1
    End_Group

    Group = Pixels
      Type       = Real
      ByteOrder  = Lsb
      Base       = 0.0
      Multiplier = 1.0
    End_Group
  End_Object

  Group = Instrument
    SpacecraftName        = "MARS GLOBAL SURVEYOR"
    InstrumentId          = MOC-WA
    TargetName            = Mars
    StartTime             = 1997-10-20T10:58:37.46
    StopTime              = 1997-10-20T11:03:44.66
    CrosstrackSumming     = 4
    DowntrackSumming      = 4
    FocalPlaneTemperature = 213.1
    GainModeId            = 1A
    LineExposureDuration  = 100.000000 <milliseconds>
    MissionPhaseName      = AB-1
    OffsetModeId          = 5
    SpacecraftClockCount  = 561812335:32
    RationaleDesc         = "OLYMPUS MONS SPECIAL RED WIDE ANGLE"
    FirstLineSample       = 673
  End_Group

  Group = Archive
    DataSetId           = MGS-M-MOC-NA/WA-2-DSDP-L0-V1.0
    ProductId           = AB-1-024/01
    ProducerId          = MGS_MOC_TEAM
    ProductCreationTime = 1999-01-15T20:40:59
    SoftwareName        = "makepds 1.3"
    UploadId            = moc_p024_v1.sasf
    ImageNumber         = 7293-024/01
    ImageKeyId          = 56181-024/01
  End_Group

  Group = BandBin
    FilterName   = RED
    OriginalBand = 1
    Center       = 0.6134 <micrometers>
    Width        = 5.0e-02 <micrometers>
  End_Group

  Group = Kernels
    NaifFrameCode       = -94032
    LeapSecond          = $base/kernels/lsk/naif0008.tls
    TargetAttitudeShape = $base/kernels/pck/pck00008.tpc
    TargetPosition      = Table
    Instrument          = $mgs/kernels/ik/moc20.ti
    SpacecraftClock     = $mgs/kernels/sclk/MGS_SCLKSCET.00060.tsc
    Frame               = Null
    InstrumentAddendum  = $mgs/kernels/iak/mocAddendum002.ti
    InstrumentPointing  = Table
    InstrumentPosition  = Table
    ShapeModel          = Null
  End_Group

  Group = Radiometry
    CalibrationKernel = /usgs/cpkgs/isis3/data/mgs/calibration/moccal.ker.001
    CoefficientFile   = $MGS/calibration/mocRedWA.coef

    /* Radiometric equation in moccal
    /* r = (pixel - z + off) / a - g / ex - dc
    a                 = 16.03
    off               = 25.0
    ex                = 100.0
    z                 = 27.67658
    dc                = 1.33691e-03
    g                 = 0.123262

    /* Reflectance = r * iof, where iof = (s * s) / w0
    w0                = 3.991
    s                 = 1.4234269469347
    iof               = 0.50767834459028
  End_Group

  Group = AlphaCube
    AlphaSamples        = 640
    AlphaLines          = 768
    AlphaStartingSample = 0.5
    AlphaStartingLine   = 0.5
    AlphaEndingSample   = 640.5
    AlphaEndingLine     = 768.5
    BetaSamples         = 640
    BetaLines           = 768
  End_Group
End_Object
