Odyssey Thermal Emission Imaging System Infrared
================================================
The Thermal Emission Imaging System (THEMIS) Infrared sensor (IR) is a linescan camera
responsible for capturing 10 infrared bands at a spatial resolution of 100
meters per pixel.


Processing THEMIS IR Images
---------------------------

Odyssey Thermal Emission Imaging System Visible
===============================================
The Thermal Emission Imaging System (THEMIS) Visible sensor (VIS) is a push frame camera
responsible for capturing 5 color bands at a spatial resolution of 18 meters
per pixel.

Processing THEMIS VIS Images
----------------------------
