Odyssey THEMIS IR
=================
The Thermal Emission Imaging System Infrared sensor is a linescan camera
responsible for capturing 10 infrared bands at a spatial resolution of 100
meters per pixel.


Processing THEMIS IR Images
---------------------------

Odyssey THEMIS VIS
==================
The Thermal Emission Imaging System Visible sensor is a push frame camera
responsible for capturing 5 color bands at a spatial resolution of 18 meters
per pixel.

Processing THEMIS VIS Images
----------------------------
