[RBlock Configuration]
-- fixed part present (yes | no)
yes
-- variable part present (yes | no)
no
[Fixed Part]
-- field 0 - dummy
0
1
0
-- field 1 - dummy
0
1
0
-- field 2
Bar ID (2 MSB)
2
none
-- field 3
PDA PHA (12 bits)
12
none
-- field 4
0
1
0
-- field 5
Bar ID (3 LSB)
3
none
-- field 6
PDB PHA (12 bits)
12
none

