=================================================
INGV definitive geomagnetic data: Castello Tesino
=================================================

.. contents:: Table of contents

1-minute averages of the components (X, Y, Z in the NEC, i.e. North-East-Center frame) and of total intensity (F) of the Earth's geomagnetic field measured at Castello Tesino magnetic observatory (IAGA code: CTS Latitude: 46.047000° Longitude: 11.649000° Altitude: 1175.000 m).  These are the definitive values that will be used to calculate GICx and GICy indices. These data are definitive, new definitive data are added yearly.
They can be retrieved from in json format from a web service so that the size of the file (estimated in the DATA DESCRIPTION TAB) actually depends on the query. Queries for a few-days data obtain a rapid reply while for longer queries (say from 1-month upward) obtain slow replies.

References
~~~~~~~~~~



Dataset summary
~~~~~~~~~~~~~~~

.. list-table::

  * - **internal_name:**
    - ingv_magdef_cts_timeseries
  * - **publisher:**
    - INGV
  * - **alph_code:**
    - 8C
  * - **id_tmp:**
    - 25
  * - **short_name:**
    - INGV_CTS_magdef
  * - **identifier:**
    - aspis:///ingv/INGV_CTS_magdef
  * - **dynamic:**
    - This peculialiar version is static being data related only to the 6 CAESAR target events, otherwise it is expected to grow.
  * - **size:**
    - 10MB
  * - **format:**
    - csv
  * - **type:**
    - timeseries
  * - **records_number:**
    - 84960
  * - **time_start:**
    - 2012-03-07
  * - **time_stop:**
    - 2017-09-15
  * - **spatial:**
    - GROUND
  * - **messenger:**
    - 
  * - **spectral_min:**
    - 1
  * - **spectral_max:**
    - 1
  * - **spectral_units:**
    - 1/minute
  * - **observable:**
    - {GIC,GEOINDEX}
  * - **latest update:**
    - 2024-03-28 05:08:11

Columns specification
~~~~~~~~~~~~~~~~~~~~~

.. list-table:: 
   :widths: 7 20 15 10 48
   :align: right 
   :header-rows: 1

   * - progr
     - column
     - units
     - type
     - description
   * - 1
     - time
     - UTC
     - datetime
     - no description
   * - 2
     - Geo_Lat
     - deg
     - float
     - Geographic Latitude °
   * - 3
     - Geo_Lon
     - deg
     - float
     - Geographic Longitude °
   * - 4
     - Altitude
     - m
     - float
     - m
   * - 5
     - X
     - nT
     - float
     - nT (X component in NEC frame)
   * - 6
     - Y
     - nT
     - float
     - nT (Y component in NEC frame)
   * - 7
     - Z
     - nT
     - float
     - nT (Z component in NEC frame)
   * - 8
     - F
     - nT
     - float
     - nT total intensity
   * - 9
     - GICx
     - dimensionless
     - float
     - no description
   * - 10
     - GICy
     - dimensionless
     - float
     - no description
   * - 11
     - AlertX
     - dimensionless
     - integer
     - Alert based on GicX index
   * - 12
     - AlertY
     - dimensionless
     - integer
     - Alert based on GicY index
