============================================================================
Worldwide GIC indices: World Data Center of Geomagnetism (WDC) observatories
============================================================================

.. contents:: Table of contents

As specified for product WDCmag, data from World Data Center of Geomagnetism observatories will be used only for the limited number of events that will be selected, so that a manual selection of the observatories and of the time period will be made. For the selected observatories GIC index (specifically GICx and GICy) will be calculated.

References
~~~~~~~~~~



Dataset summary
~~~~~~~~~~~~~~~

.. list-table::

  * - **internal_name:**
    - ingv_gic_wdc_timeseries
  * - **publisher:**
    - INGV
  * - **alph_code:**
    - 47F
  * - **id_tmp:**
    - 12
  * - **short_name:**
    - INGV_WDC_gic
  * - **identifier:**
    - aspis:///ingv/INGV_WDC_gic
  * - **dynamic:**
    - This peculialiar version is static being data related only to the 6 CAESAR target events, otherwise it is expected to grow.
  * - **size:**
    - 120MB
  * - **format:**
    - csv
  * - **type:**
    - timeseries
  * - **records_number:**
    - 1274399
  * - **time_start:**
    - 2012-03-07
  * - **time_stop:**
    - 2017-09-15
  * - **spatial:**
    - GROUND
  * - **messenger:**
    - 
  * - **spectral_min:**
    - 1
  * - **spectral_max:**
    - 1
  * - **spectral_units:**
    - 1/minute
  * - **observable:**
    - {GIC,GEOINDEX}
  * - **latest update:**
    - 2024-03-28 05:08:10

Columns specification
~~~~~~~~~~~~~~~~~~~~~

.. list-table:: 
   :widths: 7 20 15 10 48
   :align: right 
   :header-rows: 1

   * - progr
     - column
     - units
     - type
     - description
   * - 1
     - time
     - UTC
     - datetime
     - no description
   * - 2
     - IAGA_code
     - dimensionless
     - string
     - IAGA identifier of the observatory
   * - 3
     - Geo_Lat
     - deg
     - float
     - Geographic Latitude °
   * - 4
     - Geo_Lon
     - deg
     - float
     - Geographic Longitude °
   * - 5
     - Altitude
     - m
     - float
     - m
   * - 6
     - X
     - nT
     - float
     - nT (X component in NEC frame)
   * - 7
     - Y
     - nT
     - float
     - nT (Y component in NEC frame)
   * - 8
     - Z
     - nT
     - float
     - nT (Z component in NEC frame)
   * - 9
     - F
     - nT
     - float
     - nT total intensity
   * - 10
     - GICx
     - dimensionless
     - float
     - no description
   * - 11
     - GICy
     - dimensionless
     - float
     - no description
   * - 12
     - AlertX
     - dimensionless
     - integer
     - Alert based on GicX index
   * - 13
     - AlertY
     - dimensionless
     - integer
     - Alert based on GicY index
