=========================================
SAMADHA neutron dose rate at Testa Grigia
=========================================

.. contents:: Table of contents

Monitoring of the neutron dose rate due to cosmic rays at the Testa Grigia Station (3480 m, Cervinia, Italy), to study possible correlation between space weather events and dose rate at the ground. This measurement is part of the INFN project SAMADHA (South Atlantic Magnetic Anomaly Dosimetry at High Altitude) aimed to monitor the neutron dose inside the South Atlantic Anomaly (SAA) region in Bolivia. The data taken at Testa Grigia are a term of comparison for those collected in the SAA region.

References
~~~~~~~~~~

http://samadha.to.infn.it

Dataset summary
~~~~~~~~~~~~~~~

.. list-table::

  * - **internal_name:**
    - infn_tgndose_samadha_timeseries
  * - **publisher:**
    - samadha
  * - **alph_code:**
    - 75B
  * - **id_tmp:**
    - 79
  * - **short_name:**
    - TG_Ndose
  * - **identifier:**
    - aspis://infn/tgndose_samadha_timeseries
  * - **dynamic:**
    - one dataset per day (50 kB/day)
  * - **size:**
    - 50kB
  * - **format:**
    - text
  * - **type:**
    - timeseries
  * - **records_number:**
    - 2835
  * - **time_start:**
    - 2021-09-01
  * - **time_stop:**
    - 2023-12-31
  * - **spatial:**
    - GROUND
  * - **messenger:**
    - neutrons
  * - **spectral_min:**
    - 0
  * - **spectral_max:**
    - 0
  * - **spectral_units:**
    - 0
  * - **observable:**
    - {GLE,SEP,GCR}
  * - **latest update:**
    - 2024-04-04 02:15:39

Columns specification
~~~~~~~~~~~~~~~~~~~~~

.. list-table:: 
   :widths: 7 20 15 10 48
   :align: right 
   :header-rows: 1

   * - progr
     - column
     - units
     - type
     - description
   * - 1
     - time
     - UTC
     - datetime
     - datetime of the measurement
   * - 2
     - dose_rate
     - nSv/h
     - float
     - neutron ambient dose rate equivalent H*(10) average over 4 hours (nSv/h)
   * - 3
     - dose_rate_error
     - nSv/h
     - float
     - neutron dose rate measure error (nSv/h)
